win(header(pc,bprule_model_factory,'Diagnosis rules',nil),120,150,400,500,conts(`~M~J/* This knowledge base diagnoses a fault in the~M~J   main generator. By THC 12.96 */~M~J~M~JFaulty part IS power supply IF~M~J  voltage IS low .               % Defined below~M~J~M~JFaulty part IS air intake IF~M~J  power IS high AND~M~J  seal IS broken .               % Ask user to check~M~J~M~JFaulty part IS electrics IF~M~J  power IS high AND~M~J  seal IS intact AND~M~J  fuses ARE blown .              % Ask user to check~M~J~M~Jvoltage IS low if~M~J  the reading on meter 1 IS below 12 AND~M~J  the meter warning light IS off.~M~J`,'Courier New',0,16)).
